[ENV.REF.12] Cut wires

<i infocomp/envref12 0 0






Cut, sparkling wires mean the circuit is broken. In order
to move on, you'll need to close the circuit with a
conduit - an all-iron mining cart would do just fine.

[End of file]
TAGAP_END