This reactor tube will perform the final extraction of energy from a macroton.  Once all of the blue and green macrotons have reached a reactor of the same color in the machine, the energy transfer will commence.