With just how unstable the Explosive Macroton is, it cannot be held in any regular injector tube or containment unit. This highly specialized tube is constructed of the hardest metals available and keeps the Explosive Macroton centered in a magnetic field.