These injector tubes will launch the macrotons into the machine when it's activated.  As a macroton passes through the machine, its physical properties will be changed and its contained energy will be prepared for storage.