Very similar to the Junction Tube, only it rotates its direction every time a Macroton enters. The exit direction is clearly marked with arrows, and the direction it will rotate is determined by the circular arrow in the center.