<l><5>Mercury Outboards
<l><5>- Propshaft
<l><5>Horsepower:135-hp
<l><5>(1000kW)
<l><5>-Max RPM(W.O.T):
<l><5>5000-5600
<l><5>-Cylinders/
<l><5>Configuration:
<l><5>60 degree V-6
<l><5>-Displacement: 
<l><5>153 cu.in.(2500cc)
<l><5>-Bore & Sroke: 3.5in.
<l><5>x 2.65 in.(89mm x
<l><5>67mm)
<l><5>-Fuel Induction
<l><5>System:2Stage Direct
<l><5>- Fuel injection
<l><5>-Exhaust Sustem:
<l><5>  Trought Prop
<l><5>-Lubrication System:
<l><5>Electronic multi-point
<l><5>variable ratio oil
<l><5>injection
<l><5>-Cooling System
<l><5>Watrer cooled with
<l><5>thermostat and
<l><5>pressure controlled
<l><5>-Ignition System:
<l><5>Digital Inductive
<l><5>-Starting System:
<l><5>Electric(turnkey)
<l><5>-Alternator:
<l><5>Belt-driven 60 amp
<l><5>(756 watt) with
<l><5>voltage regulator
<l><5>-Gear Ratio: 2.0:1
<l><5>-Gear Shift: F-N-R
<l><5>-Steering: Remote
<l><5>-Trim System: Power
<l><5>trim
<l><5>- Shaft Lenght: 20 in.
<l><5>(508mm)
<l><5>-Weight-Dry:433lbs.
<l><5>(201kg) 
<l><5>-Operator warning
<l><5>Systems: Overheat,
<l><5>low oil level, water 
<l><5>in fuel, check engine.
<l><5>-Propeller Options:
<l><5>Black Max,
<l><5>Vengeance, Laser II,
<l><5>Mirage Plus, Tempest 
<l><5>Plus, Trophy Plus,
<l><5>High Five.
